# Static Timing Analysis

Project : | PSoC4_LED_FreeRTOS
Build Time : | 06/07/15 15:44:11
Device : | CY8C4245AXI-483
Temperature : | -40C - 85C
VDDA : | 3.30
VDDD : | 3.30
Voltage : | 3.3

Expand All | Collapse All | Show All Paths | Hide All Paths
+ Timing Violation Section
No Timing Violations
+ Clock Summary Section

Clock | Domain | Nominal Frequency | Required Frequency | Maximum Frequency | Violation
--- | --- | --- | --- | --- | ---
CyHFCLK | CyHFCLK | 48.000 MHz | 48.000 MHz | N/A |
CyILO | CyILO | 32.000 kHz | 32.000 kHz | N/A |
CyIMO | CyIMO | 48.000 MHz | 48.000 MHz | N/A |
CyLFCLK | CyLFCLK | 32.000 kHz | 32.000 kHz | N/A |
CyRouted1 | CyRouted1 | 48.000 MHz | 48.000 MHz | N/A |
CySYSCLK | CySYSCLK | 48.000 MHz | 48.000 MHz | N/A |